## DTC Troubleshooting: 14-1, 14-2

DTC 14-1, 14-2: | Internal Failure of the Front Passenger's Side Impact Sensor

1. | Erase the DTC memory.

2. | Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on? YES - Replace the front passenger's side impact sensor.n NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures.