## Climate Control Unit Removal and Installation

NOTE: LHD type is shown, RHD type is symmetrical.

1. | Remove the center panel.

2. | Remove the audio unit or the navigation unit.

3. | Remove the self-tapping screws and the heater control unit (A).

4. | Install the control unit in the reverse order of removal. After installation, operate the control unit controls to see whether it works properly.