## Tailgate Key Cylinder Switch Test

1. | Remove the tailgate trim panel.

2. | Open the tailgate.

3. | Disconnect the 3P connector from the key cylinder switch.

4. | Check for continuity between the terminals. There should be continuity between the No. 2 and No. 3 terminals when the tailgate key cylinder switch is LOCK position. There should be continuity between the No. 1 and No. 2 terminals when the tailgate key cylinder switch is UNLOCK position.