## DTC Troubleshooting: P0560 (34)

DTC P0560: | ECM Power Source Circuit Malfunction

1. | Turn the ignition switch ON (II).

2. | Do the DTC CLEAR in the CLEAR MENU with the HDS.

3. | Start the engine.

4. | Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Is DTC P0560 indicated? YES - Substitute a known-good ECM and recheck. If symptom/indication goes away, replace the original ECM.n NO - Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the PGM-FI main relays and the ECM.n