## Ignition Switch Test

SRS components are located in this area. Review the SRS component locations, and precautions and procedures in the SRS section before performing repairs or servicing.

1. | Remove the battery negative cable.

2. | Remove the steering column cover's.

3. | Check for continuity between the terminals in each switch position according to the table.

4. | If the continuity checks do not agree with the table, replace the steering lock assembly.