## High/Low Beam Switching Solenoid Test

1. | Remove the headlight.

2. | Remove the HID bulb from the headlight.

3. | Disconnect the 2P connector (A) from the high/low beam switching solenoid (B).

4. | Check the hood of the high/low beam switching solenoid. The hood should open (high beam) when the battery power is connected to the No. 1 terminal and ground the No. 2 terminal. The hood should close (low beam) when the battery power is disconnected.

5. | If the solenoid does not work properly, replace it.