## ATF Replacement

NOTE: Keep all foreign particles out of the transmission.

1. | Park the vehicle on level ground.

2. | Remove the drain plug (A), and drain the automatic transmission fluid (ATF).

3. | Reinstall the drain plug with the new sealing washer (B).

4. | Refill the transmission with genuine Honda ATF-Z1 Automatic Transmission Fluid (ATF) into the dipstick guide pipe opening (A) to the upper mark on the dipstick. Always use genuine Honda ATF-Z1, using a non-Honda ATF can affect the shift quality.
Automatic Transmission Fluid Capacity:
3.2 L (3.4 US qt, 2.8 Imp qt) at change
5.4 L (5.7 US qt, 4.8 Imp qt) at overhaul

5. | Check the fluid level. It should be between upper mark (B) and lower mark (C) on the COLD gauge.

6. | Insert the dipstick back into its guide pipe.