## Dashboard Center Vent Removal/Installation

1. | Wrap a flat-tip screwdriver with protective tape, and apply protective tape around the related parts to prevent damage. Carefully insert a flat-tip screwdriver next to the outside pivot, and pry the center vent (A) out. Take care not to scratch the dashboard and related parts.

2. | If any bushing (B) dropped from each pivot of the center duct while removing the center vents, reinstall it onto the pivot.

3. | Set the outside pivot portion of the center vent on the bushing first, then push the opposite side into place securely.