## ATF Feed Pipe Replacement - Flywheel Housing

1. | Remove the snap ring (A), then remove the ATF feed pipe (B) and feed pipe flange (C).

2. | Replace the ATF feed pipe, and install the new ATF feed pipe by aligning its tab (D) with the guide on the housing.

3. | Install the new O-ring (E) over the feed pipe, and install the new O-ring (F) in the feed pipe flange, then install the feed flange over the feed pipe.

4. | Secure the feed pipe in the housing with the snap ring.