### Maintenance Schedule for Severe Conditions - European Model

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling or long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 10,000 km (6,250 miles) or 6 months
Replace engine oil filter | l | l | l | l | l | l | l | l | l | l
Clean air cleaner element Use the Normal Conditions except in dusty conditions | Dry type only | Every 20,000 km (12,500 miles)
Replace air cleaner element Use the Normal Conditions except in dusty conditions | Dry type | Every 40,000 km (25,000 miles)
Wet type | Every 20,000 km (12,500 miles)
Inspect the valve clearance Check valve clearance |  | l |  | l |  | l |  | l |  | l
Replace fuel filter |  |  |  |  |  | l |  |  |  |
Replace spark plugs | Every 40,000 km (25,000 miles)
Inspect and adjust drive belts Check for cracks, damage Check deflection and tension |  | l |  | l |  | l |  | l |  | l
Inspect idle speed L12A4 and L13A6 (with ETCS) engines, L13A6 (without ETCS) engine |  |  |  |  |  | l |  |  |  |
Replace engine coolant Use Genuine Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years
Replace transmission fluid (MTF) Use Honda MTF (Manual Transmission Fluid) | Every 60,000 km (37,500 miles) or 4 years
Replace CVT fluid (ATF) Use Honda ATF-Z1 Change CVT fluid (ATF-Z1) every 40,000 km (25,000 miles) or 2 years if you drive at high speed in extremely hot over 35 °C (95 °F) condition |  |  |  | l |  |  | l |  |  | l
Inspect front and rear brakes Check the front brake pad and disc thickness. Check for damage and cracks front brake pad, front brake disc Check the rear brake pad and disc thickness. Check for damage and cracks rear brake pad, rear brake disc Check the wheel cylinder for leaks Check the brake linings for cracking, glazing, wear, and contamination Check the front brake caliper for damage, leaks, and tightness Check the rear brake caliper for damage, leaks, and tightness | Every 10,000 km (6,250 miles) or 6 months
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid (We recommend Genuine Honda Brake Fluid). Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Check parking brake adjustment, drum brake, disc brake Check the parking brake operation | l | l | l | l | l | l | l | l | l | l
Replace dust and pollen filter | Every 30,000 km (18,750 miles) or 1 year
Check lights alignment Check the position of the headlights | l | l | l | l | l | l | l | l | l | l
Test drive (Check for noise, road stability, vibrations, and dashboard operations) | l | l | l | l | l | l | l | l | l | l
Visually inspect the following items Check for correct installation and position, check for cracks, deterioration, rust, and leaks Check tightness of screws, nuts, and joints. If necessary, retighten
Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage Check the boot for damage and leaking grease | Every 10,000 km (6,250 miles) or 6 months
Suspension components Check the bolts for tightness Check all dust cover for deterioration and damage
Driveshaft boots Check boot and boot band for cracks Check rack grease
Brake hoses and lines (including ABS/VSA) Check the master cylinder, proportioning control valve, and ABS or VSA modulator for damage and leakage | l | l | l | l | l | l | l | l | l | l
All fluid levels and condition of fluid Engine coolant MTF ATF Brake fluid Windshield washer fluid
Exhaust system Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration Retighten loose connections and replace any damaged parts
Tyre condition Check for pressure, puncture or cuts and irregular thread wear