### Maintenance Schedule for Normal Conditions - Except European, Australian and New Zealand Models

Follow the Normal Conditions Maintenance Schedule if the servere driving conditions specified in the Servere Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Clean air cleaner element | Dry type only | Every 10,000 km (6,250 miles)
Replace air cleaner element | Wet type | Every 20,000 km (12,500 miles)
Dry type | Every 20,000 km (12,500 miles)
Inspect the valve clearance Check valve clearance | Every 40,000 km (25,000 miles)
Replace fuel filter For replacement infomation under driving condition The fuel filter should be replaced according to the time and distance recommendations in the maintenance schedule. It is recommended to replace the fuel filter every 40,000 km (25,000 miles) or 2 years (except EU model), if the fuel you are using is suspected to be contaminated with dust, etc. Because the filter may be clogged sooner. Have a qualified technician change the fuel filter. Since the fuel system is under pressure, fuel can spray out and create a hazard if all fuel line connections are not handled correctly. |  |  |  | l |  |  |  | l |  |
Replace spark plugs | Every 40,000 km (25,000 miles)
Inspect and adjust drive belts Check for cracks, damage. Check deflection and tension. |  | l |  | l |  | l |  | l |  | l
Inspect idle speed |  |  |  |  |  | l |  |  |  |
Replace engine coolant Use Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then replace every 100,000 km (60,000 miles) or 5 years
Replace transmission fluid (MTF) Use Honda MTF (Manual Transmission Fluid) |  |  |  |  |  | l |  |  |  |
Replace CVT fluid (ATF) Use the Honda ATF-Z1 |  |  |  | l |  |  | l |  |  | l
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage and cracks brake pad, brake disc. Check the wheel cylinder for leaks. Check the brake linings for cracking, glazing, wear, and contamination. Check the calipers for damage, leaks, and tightness. | Every 10,000 km (6,250 miles) or 6 months
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid (We recommend Honda Brake Fluid). Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Check parking brake adjustment Check the parking brake operation | l | l |  | l |  | l |  | l |  | l
Rotate tyres (Check tyre inflation and condition at least once per month) | Every 10,000 km (6,250 miles)
Visually inspect the following items Check for correct installation and position, check for cracks, deterioration, rust, and leaks. Check tightness of screws, nuts, and joints. If necessary, retighten.
Tie rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease. | Every 10,000 km (6,250 miles) or 6 months
Suspension components Check the bolts for tightness. Check all dust cover for deterioration and damage.
Driveshaft boots Check boot and boot band for cracks. Check rack grease.
Brake hoses and lines (including ABS) Check the master cylinder, proportioning control valve, and ABS modular for damage and leakage | l | l | l | l | l | l | l | l | l | l
All fluid levels and condition of fluid Engine coolant. MTF. ATF. Brake fluid. Windshield washer.
Exhaust system Check the catalytic converter heat shield, exhaust pipe, and muffler for damage. leaks and tightness
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts.