## Tailgate Light Test/Replacement

1. | Open the tailgate.

2. | Carefully pry out the tailgate light (A).
Side Turn Signal Light: | 5W

3. | Disconnect the 2P connector (B) from the light.

4. | Check for continuity between the No. 1 (+) and No. 2 (-) terminals with the light switch ON. There should be continuity. If there is no continuity, check the bulb. If the bulb is OK, replace the tailgate light.