## Audio Unit Connector Replacement

Cavity | Wire | Connects to | Cavity | Wire | Connects to
--- | --- | --- | --- | --- | ---
1 | ——— | Not used | 11 | ——— | Not used
2 | YEL/RED | ACC (Main stereo power supply) | 12 | ——— | Not used
3 | ——— | Not used | 13 | ——— | Not used
4 | ——— | Not used | 14 | ——— | Not used
5 | PNK | Right rear door speaker (+) | 15 | BLU/YEL | Right rear door speaker (-)
6 | BLU/WHT | Left rear door speaker (+) | 16 | BLU/BLK | Left rear door speaker (-)
7 | GRN/YEL | Right front door speaker (+) | 17 | GRY/RED | Right front door speaker (-)
8 | GRN/BLK | Left front door speaker (+) | 18 | LT GRN | Left front door speaker (-)
9 | RED/BLK | Lights-on signal | 19 | ——— | Not used
10 | WHT/RED | Constant power | 20 | BLK | Ground (G403)