## 7-speed Mode Main Switch Test

## For KB, KE, KG, and KQ (L15A1 engine) Models (6-position CVT+7Speed Mode)

SRS components are located in this area. Review the following articles in the SRS before performing repairs or service;

- Component Locations.
- Precautions and Procedures.

1. | Remove the steering wheel.

2. | Check the 7SPEED MODE main switch for continuity between cable reel subharness 13P connector terminals No. 8 and No. 9. There should be toggled continuity and no continuity between terminals every time the main switch pushes.

3. | 7SPEED MODE main switch test has finished if the test result is OK. If the main switch works incorrectly at the 13P connector, test the switch at the switch connector.

4. | Remove the screws (A) (4) securing the steering wheel rear cover (B), then remove the steering wheel rear cover.

5. | Remove steering shift + (plus) switch connector from its clamp, then disconnect the connector.

6. | Remove the screw (C) securing the steering shift + (plus) switch (D), then remove the switch.

7. | Disconnect 7SPEED MODE main switch connector (E), and remove the 7SPEED MODE main switch assembly (F).

8. | Check the 7SPEED MODE main switch for continuity between the switch connector terminals No. 5 and No. 6. There should be toggled continuity and no continuity between terminals every time the main switch pushes.

9. | Replace the 7SPEED MODE main switch assembly if the main switch works incorrectly.

10. | Replace the cable reel subharness if the main switch is OK.