## Radiator Fan Switch Replacement

1. | Drain the engine coolant.

2. | Remove the air cleaner housing.

3. | Disconnect the radiator fan switch connector, then remove the radiator fan switch (A).

4. | Install the radiator fan switch with a new O-ring (B).

5. | Clean up any spilled engine coolant.

6. | Install the air cleaner housing.

7. | Refill the radiator with engine coolant, and bleed air from the cooling system with the heater valve open.