## DTC Troubleshooting: 67

DTC 67: | Brake Pedal Position Switch (Hardwear)

1. | Check the brake pedal position switch. Is the switch OK? YES - Go to 2. NO - Replace the brake pedal position switch.n

2. | Disconnect the VSA control unit 46P connector.

3. | Turn the ignition switch ON (II).

4. | Measure the voltage between body ground and the VSA control unit 46P connector terminal No. 6 when the brake pedal is released. Is there battery voltage? YES - Repair short to power in the wire between the VSA control unit and under-hood fuse/relay box.n NO - Replace the VSA modulator-control unit.n