## Fuel Pressure Test

Special Tools Required
Fuel pressure gauge ( 07406-0040002)

Fuel pressure gauge set ( 07ZAJ-S5A0100)

1. | Relieve the fuel pressure.

2. | Disconnect the quick-connect fitting. Attach the fuel pressure gauge set and fuel pressure gauge.

3. | Start the engine and let it idle. If the engine starts, go to 5. If the engine does not start, go to 4.

4. | Check to see if the fuel pump is running: listen to the fuel fill port with the fuel fill cap removed. The fuel pump should run for 2 seconds when the ignition switch is first turned on. If the pump runs, 5. If the pump does not run, do the fuel pump circuit troubleshooting.

5. | Read the pressure gauge. The pressure should be 320-370 kPa (3.3-3.8 kgf/cm2, 47-54 psi) If the pressure is OK, the test is complete. If the pressure is out of specification, replace the fuel pressure regulator, and the fuel filter, then recheck the fuel pressure.