## Engine Oil Pan Installation

1. | Remove old liquid gasket from the oil pan mating surfaces, bolts and bolt holes.

2. | Clean and dry the oil pan mating surfaces.

3. | Install the new oil pan gasket on the oil pan.

4. | Apply liquid gasket, P/N 08C70-K0334M or 08C70- X0331S, to the cylinder block mating surface of the oil pan and the inner threads of the holes. #### NOTE: Apply a 1.5 mm wide bead of the liquid gasket along the broken line (A). Apply a 5.0 mm wide bead of the liquid gasket to the shaded area (B). Do not install the parts if 5 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue.

5. | Install the oil pan (A) with dowel pin (B) and new O-ring (C).

6. | Tighten the bolts in two or three steps.
Specified torque:
(1): | 24 N·m (2.4 kgf·m, 17 lbf·ft)
(2)-(13): | 12 N·m (1.2 kgf·m, 8.7 lbf·ft)

7. | Install the clutch cover/torque converter cover (A), and tighten the two bolts (B) securing the transmission.

8. | Install the dipstick tube (A) with new O-ring (B).

9. | After assembly, wait at least 30 minutes before filling the engine with oil.