## SRS Unit Replacement

## Removal

1. | Disconnect the battery negative cable, and wait at least 3 minutes before beginning work.

2. | Disconnect the driver's and front passenger's airbag connectors.

3. | Disconnect the side airbag connectors.

4. | Disconnect both seat belt tensioner connectors.

5. | Remove the center console.

6. | Pull down the carpet, then disconnect the connectors and remove the two Torx bolts (A), then pull out the SRS unit (B) from the right side.

## Installation

1. | Install the new SRS unit (A) with Torx bolts (B), then connect the connectors (C) to the SRS unit; push it into position until it clicks. NOTE: When tightening the Torx bolts to the specified torque after replacement, be careful to turn them in so that their heads rest squarely on the brackets.

2. | Reinstall the center console.

3. | Reconnect the driver's and front passenger's airbag connectors.

4. | Reconnect the side airbag connectors.

5. | Reconnect both seat belt tensioner connectors.

6. | Reconnect the battery negative cable.

7. | Initialize the OPDS unit.

8. | After installing the SRS unit, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.