## Camshaft Sprocket Installation

NOTE: Keep the cam chain away from magnetic fields.

1. | Install the cam chain to the camshaft sprocket by alignment the reference mark (A), then install the camshaft sprocket on the camshaft.

2. | Hold the camshaft with an open-end wrench, then tighten the bolt.
Specified torque:
56 N·m (5.7 kgf·m, 41 lbf·ft)

3. | Apply engine oil to the slider surface of the cam chain tensioner slider through the oil return hole in the cylinder head.

4. | Hold the crankshaft pulley and set the socket wrench (A) on the camshaft sprocket bolt.

5. | Turn the camshaft clockwise to compress the cam chain tensioner, then remove the 6 x 1.0 mm bolt (B). NOTE: Turning torque should not exceed 56 N·m (5.7 kgf·m, 41 lbf·ft), when turning the camshaft. Do not turn the camshaft counterclockwise.

6. | Install the maintenance bolt (C) with a new washer (D).

7. | Install the new cylinder head plug.

8. | Install the cylinder head cover.