## Rocker Arm Assembly Installation

1. | Install the rocker arm assembly (A) with dowel pin (B). NOTE: When reassembling the rocker arms, Install the rocker arm from cam chain side on the rocker shaft.

2. | Tighten each bolts two turns at a time in sequence below.
Specified torque:
29 N·m (3.0 kgf·m, 22 lbf·ft)
Apply engine oil to the bolt threads and flange

3. | Adjust the valve clearance.

4. | Install the cylinder head cover.