## Hood Release Handle Replacement

1. | Remove the kick panel.

2. | Remove the bolts, then remove the hood release handle (A).

3. | Disconnect the hood opener cable (B) from the hood release handle. Take care not to bend the cable.

4. | Install the hood release handle in the reverse order of removal, and note there items: Make sure the hood opener cable is connected properly. Make sure the hood opens properly.