## Steering Rack Guide Replacement

## Manufactored in except HATC

NOTE: During removal/installation, do not allow dust, dirt, or other foreign materials to enter the gearbox.

1. | Loosen the locknut (A), then remove the rack guide screw (B), conical springs (C), holder (D), needle roller (E), and roller (F) from the steering gearbox.

2. | Grease the inside of holder and the sliding surface and circumference of the roller.

3. | Install the roller, the needle roller, and the holder onto the gearbox housing. Wipe the grease off the threaded section (G) of the housing.

4. | Install the conical springs onto the holder. NOTE: Make sure the number of the conical springs and the direction when installing.

5. | Apply sealant to the threads on the rack guide screw, then install and tighten it to 25 N·m (2.5 kgf·m, 18 lbf·ft). Loosely install the locknut.

6. | Adjust rack guide screw. After adjusting, check that the rack moves smoothly by sliding it right and left.