## CVT Control Shaft Removal/Inspection

1. | Remove the bolt (A) and lock washer (B), then remove the control lever (C) from the control shaft (D).

2. | Remove the control shaft from the transmission housing.

3. | Check for fluid leaks between the housing and oil seal (E). If there is a fluid leak, replace the oil seal with a new one.

4. | Install the control shaft in the transmission housing, and install the control lever on the control shaft.

5. | Install the lock bolt with the new lock washer.