## DTC Troubleshooting: 75

DTC 75: | Lateral Acceleration Sensor (Joint Failure)

1. | Check the installation condition of the yaw rate/lateral acceleration sensor. Is it correctly installed? YES - Go to 2. NO - If the loose the mounting bolts, tighten the mounting bolts properly, and recheck.n

2. | Park the vehicle on a level surface. Check YAW RATES LATERAL in the DATA LIST with the HDS. Is the result? YES - Check for loose connector terminals in the VSA control unit 46P connector and repair if necessary. If terminals are OK, replace the VSA modulator-control unit.n NO - Replace the yaw rate/lateral acceleration sensor.n