## Cable Reel Subharness Replacement - With 7-speed Mode

## For KB, KE, KG, and KQ (L15A1 engine) Models (6-position CVT+7Speed Mode)

SRS components are located in this area. Review the following articles in the SRS before performing repairs or service;

- Component Locations.
- Precautions and Procedures.

1. | Remove the steering wheel.

2. | Remove the screws (A) (4) securing the steering wheel rear cover (B), then remove the steering wheel rear cover.

3. | Remove steering shift + (plus) switch connector from its clamp, and disconnect the connector.

4. | Remove the screw (C) securing the steering shift + (plus) switch (D), then remove the steering shift + (plus) switch and 7SPEED MODE main switch (E).

5. | Disconnect 7SPEED MODE main switch connector.

6. | Remove the steering shift - (minus) switch connector (A) from its clamp, and disconnect the connector. Disconnect audio remote control switch connector if equipped.

7. | Remove the harness guide (B) and cable reel subharness (C), and remove the cable reel subharness from the harness guide.

8. | Replace the cable reel subharness, and install the new subharness on the harness guide.

9. | Install the harness guide on the steering wheel.

10. | Install the 7SPEED MODE main switch and steering shift + (plus) switch with the screw, and install the steering wheel rear cover with the screws (4).

11. | Connect disconnected connectors.

12. | Install the steering wheel.