## Cylinder Head Cover Installation

1. | Thoroughly clean the head cover gasket and the groove.

2. | Install the head cover gasket (A) in the groove of the cylinder head cover (B).

3. | Check that the mating surfaces are clean and dry.

4. | Apply a 3.0 mm wide bead of the liquid gasket, P/N 08C70-K0234M, 08C70-K0334M or 08C70-X0331S, on the chain case mating areas (A). NOTE: Do not install the parts if 5 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue.

5. | Once the cylinder head cover (A) on the cylinder head, slide the cover slightly back and forth to seat the head cover gasket.

6. | Inspect the cover washer (B). Replace any washer that is damaged or deteriorated.

7. | Tighten the bolts in two or three steps. In the final step tighten all bolts, in sequence, 12 N·m (1.2 kgf·m, 8.7 lbf·ft).

8. | Install the harness bracket mounting bolt (A), breather hose (B) and ground cable (C).

9. | Install the eight ignition coils.

10. | Install the intake manifold.

11. | Check that all tubes, hoses, and connectors are installed correctly.

12. | After assembly, wait at least 30 minutes before filling the engine with oil.