## Climate Control Unit Disassembly and Reassembly

1. | Widen the cable stops (A) in the cable holder (B) using a snap ring pliers, then pull out the recirculation control cable (C). Remove the self-tapping screws and the control module (D).

2. | Hook the tip of the new control cable to the lever, then push the cable housing into the cable holder until it locks into place.

3. | After assembly, check that the lever slides or the dial turns smoothly through the full storke from right to left.