### Maintenance Schedule for Severe Conditions - European Model

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions: Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip. Driving in extremely hot over 35 °C (95 °F) conditions. Extensive idling, or long periods of stop-and-go-driving. Trailer towing, driving with a car-top carrier, or driving in mountainous conditions. Driving on muddy, dusty, or de-iced roads.

If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 10,000 km (6,000 miles) or 6 months
Replace engine oil filter | l | l | l | l | l | l | l | l | l | l
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage and cracks Check the wheel cylinder for leaks Check the brake linings for cracking, glazing, wear and contamination Check the calipers for damage, leaks, and tightness | Every 10,000 km (6,000 miles)or 6 mounths
Check parking brake adjustment | l | l | l | l | l | l | l | l | l | l
Check lights alignment Check the position of the headlights | l | l | l | l | l | l | l | l | l | l
Test drive (noise, stability, dashboard operation) Check for road stability, noise, vibration and dashboard operation. | l | l | l | l | l | l | l | l | l | l
Visually inspect the following items: Check for correct installation and position, check for cracks, deterioration, rust, and leaks. Check tightness of screws, nuts, and joints. If necessary, retighten.
Tie rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease | Inspect every 10,000 km (6,000 miles) or 6 months
Suspension components Check the bolts for tightness Check all dust cover for deterioration and damage
Driveshaft boots Check the boot and boot band for cracks Check rack grease

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Brake hoses and lines (including ABS) Check the master cylinder, proportioning control valve and ABS modulator and leakage | l | l | l | l | l | l | l | l | l | l
All fluid levels and condition fluid Check levels and check for leaks. If necessary, add engine coolant MTF, ATF,brake fluid, windshield fluid, and battery fluid.
Exhaust system Check the exhaust pipe and muffler for damage, leaks and tightness
Fuel lines and connections Check fuel lines for loose connections, cracks and deterioration. Retighten loose connections and replace any damaged parts
Tyre condition Check for pressure, puncture, cuts, and irregular thread wear.
Replace air cleaner element | l | l | l | l | l | l | l | l | l | l
Replace spark plugs | Every 40,000 km (24,000 miles)
Inspect valve clearance
Inspect and adjust drive belts Check for cracks, damage, deflection and tension |  | l |  | l |  | l |  | l |  | l
Replace dust and pollen filter | Every 30,000 km (18,000 miles) or 1 year
Replace fuel filter |  |  |  |  |  | l |  |  |  |
Inspect idle speed |  |  |  |  |  | l |  |  |  |
Replace manual transmission fluid Use genuine Honda Manual Transmission Fluid (MTF) | Every 60,000 km (36,000 miles) or 4 years
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then replace every 100,000 km (60,000 miles) or 5 years
Replace brake fluid Use only DOT 3 brake fluid (We recommend Genuine Honda Brake Fluid). Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years