## Inhibitor Solenoid Test

1. | Disconnect the inhibitor solenoid connector.

2. | Measure inhibitor solenoid resistance at the connector terminals.
STANDARD: | 11.7-21.0 W

3. | Replace the inhibitor solenoid if the resistance is out of standard.

4. | If the resistance is within the standard, connect the battery positive terminal to inhibitor solenoid connector terminal No. 2, and connect the battery negative terminal to the connector terminal No. 1. A clicking sound should be heard. Replace the inhibitor solenoid if no clicking sound is heard.