## CVT Differential Carrier Bearing Side Clearance Inspection

Special Tools Required
Driver 40 mm I.D. ( 07746-0030100)

1. | Install the set ring in the transmission housing.

2. | Install the differential assembly in the transmission housing, then drive the differential to seat in the housing.

3. | Install the dowel pins (3) (A) and gasket (B) on the transmission housing (C).

4. | Place the flywheel housing (D) on the transmission housing.

5. | Install the housing bolts, and tighten them in a crisscross pattern in two or more steps.

6. | Measure the clearance between the set ring and carrier bearing outer race with a feeler gauge.
STANDARD: | 0-0.15 mm (0-0.006 in.)

7. | If the clearance is out of standard, remove the set ring, and measure its thickness.

8. | Select a new set ring from the following table.
SET RING, 80 mm
No. | Part Number | Thickness
--- | --- | ---
1 | 90414-689-000 | 2.5 mm (0.098 in.)
2 | 90415-689-000 | 2.6 mm (0.102 in.)
3 | 90416-689-000 | 2.7 mm (0.106 in.)
4 | 90417-689-000 | 2.8 mm (0.110 in.)
5 | 90418-689-000 | 2.9 mm (0.114 in.)
6 | 90419-PH8-000 | 3.0 mm (0.118 in.)

9. | Install the new set ring, and rechck the clearance and make sure it is within the standard.