## Power Relays Test - Normally-open Type A

Use this chart to identify the type of relay, then do the test listed for it.

Relay | Test
--- | ---
A/C compressor clutch relay | Normally-open type A
A/T reverse relay
Blower motor relay
Condensor fan relay
Headlight relay
Horn relay
Left HID headlight relay
Right HID headlight relay
Left activation indicator relay
Right activation indicator relay
PGM-FI main relay 1
PGM-FI main relay 2
Power mirror defogger relay
Power window relay
Radiator fan relay
Rear window defogger relay
Starter cut relay
Taillight relay
EPS motor relay | Normally-open type B
Power door lock/fuel lid lock relay | Five terminal type
Power door unlock/fuel lid unlock relay
Sunroof open relay
Sunroof close relay
Left super locking relay
Right super locking relay

## Normally-open type A

Check for continuity between the terminals.

- There should be continuity between the No. 1 and No. 2 terminals when power and ground are connected to the No. 3 and No. 4 terminals.
- There should be no continuity between the No. 1 and No. 2 terminals when power is disconnected.

type 1:

type 2:

### · PGM-FI main relay 1
· PGM-FI main relay 2

type 1:

type 2: