## Control Valve Body Replacement

1. | Remove the air cleaner housing and intake air duct.

2. | Disconnect the inhibitor solenoid connector (A) and CVT drive pulley speed sensor connector (B).

3. | Disconnect the CVT start clutch pressure control valve connector (A), CVT pulley pressure control valve connector (B) and CVT speed change control valve connector (C).

4. | Remove the bolt (D) securing the harness cover (E), pull the harness cover, and remove it from its bracket (F).

5. | Remove the battery cable clamps (A) from their brackets (B).

6. | Remove the radiator hose from its clamp (C), and remove the radiator hose clamp.

7. | Remove the control valve body, and replace it.

8. | Install new O-rings (A) on the ATF pipes (B), and install them in the transmission housing.

9. | Install the new control valve body (C) over the ATF pipes with the new gasket (D) and dowel pins (E).

10. | Install removed parts in the reverse order of removal.