## MTF Inspection and Replacement

1. | Park the vehicle on level ground, and turn the engine OFF.

2. | Remove the oil filler plug (A) and washer (B), check the condition of the fluid, and make sure the fluid is at the proper level (C).

3. | If the transmission fluid is dirty, remove the drain plug (D) and drain the fluid.

4. | Reinstall the drain plug with a new washer, and refill the transmission fluid to the proper level.
Oil Capacity
| 1.5 [liter] (1.6 US qt, 1.3 lmp qt) at fluid change
| 1.6 [liter] (1.7 US qt, 1.4 lmp qt) at overhaul
Always use Genuine Honda Manual Transmission Fluid (MTF). Using motor oil can cause stiffer shifting because it does not contain the proper additives.

5. | Reinstall the oil filler plug with a new washer.