### Maintenance Schedule for Normal Conditions - Australian and New Zealand Models

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 10,000 km (6,250 miles) or 1 year
Replace engine oil filter | l | l | l | l | l | l | l | l | l | l
Replace air cleaner element |  | l |  | l |  | l |  | l |  | l
Inspect the valve clearance Check valve clearance |  | l |  | l |  | l |  | l |  | l
Replace fuel filter |  |  |  | l |  |  |  | l |  |
Replace spark plugs | L13A1 engine (Normal type) |  | l |  | l |  | l |  | l |  | l
L15A1 engine (Iridium type) |  |  |  |  | l |  |  |  |  | l
Inspect and adjust drive belts Check for cracks, damage Check deflection and tension |  | l |  | l |  | l |  | l |  | l
Inspect idle speed |  |  |  |  | l |  |  |  |  | l
Replace engine coolant Use Genuine Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years
Replace transmission fluid (MTF) Use Honda MTF (Manual Transmission Fluid) |  |  |  |  |  | l |  |  |  |
Replace CVT fluid (ATF) Use Honda ATF-Z1 |  |  |  | l |  |  | l |  |  | l
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage and cracks brake pad, brake disc Check the wheel cylinder for leaks Check the brake linings for cracking, glazing, wear, and contamination Check the calipers for damage, leaks, and tightness | l | l | l | l | l | l | l | l | l | l
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid (We recommend Genuine Honda Brake Fluid). Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Check parking brake adjustment Check the parking brake operation | l | l |  | l |  | l |  | l |  | l
Check lights alignment Check the position of the headlights | l | l | l | l | l | l | l | l | l | l
Test drive (Check for noise, road stability, vibrations, and dashboard operations) | l | l | l | l | l | l | l | l | l | l
Rotate tyres (Check tyre inflation and condition at least once per month) | Every 10,000 km (6,250 miles) or 1 year
Visually inspect the following items Check for correct installation and position, check for cracks, deterioration, rust, and leaks Check tightness of screws, nuts, and joints. If necessary, retighten
Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage Check the boot for damage and leaking grease | l | l | l | l | l | l | l | l | l | l
Suspension components Check the bolts for tightness Check all dust cover for deterioration and damage
Driveshaft boots Check boot and boot band for cracks Check rack grease
Brake hoses and lines (including ABS/VSA) Check the master cylinder, proportioning control valve, and ABS or VSA modulator for damage and leakage
All fluid levels and condition of fluid Engine coolant MTF ATF Brake fluid Windshield washer fluid
Exhaust system Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration Retighten loose connections and replace any damaged parts