## DTC Troubleshooting: 31, 32, 33, 34, 35, 36, 37, 38

DTC 31, 32, 33, 34, 35, 36, 37, 38: | ABS Solenoid

1. | Clear the DTCs using the HDS.

2. | Turn the ignition switch ON (II).

3. | Check the DTCs using the HDS. Does the ABS indicator come on, and are DTCs 31, 32, 33, 34, 35, 36, 37 38 indicated? YES - Check for loose or poor connections in the VSA control unit 46P connector. If connections are good, replace the VSA modulator-control unit.n NO - The system is OK at this time.n