## Driveshafts Installation

1. | Install a new set ring onto the set ring groove of the driveshaft (left driveshaft).

2. | Install the outboard joint (A) into the front hub (B).

3. | Install the knuckle (A) onto the lower arm (B). Be careful not to damage the ball joint boot (C). Wipe off the grease before tightening the nut at the ball joint. Torque the castle nut (D) to the lower torque specification, then tighten it only far enough to align the slot with the pin hole. Do not align the nut by loosening.

4. | Install the new lock pin (E) into the pin hole from the inside of the vehicle.

5. | Install the heat cover. NOTE: Tighten the three bolts in number of the order.

6. | Install a new spindle nut (A), then tighten the nut. After tightening, use a drift to stake the spindle nut shoulder (B) against the driveshaft.

7. | Clean the mating surfaces of the brake disc and the front wheel, then install the front wheel with the wheel nuts.

8. | Refill the transmission with recommended transmission fluid: Manual transmission CVT

9. | Check the front wheel alignment, and adjust it if necessary.