## Windshield Wiper Intermittent Control Circuit Input Test

1. | Remove the wiper/washer switch. LHD type and KE model: RHD type except KE:

2. | With the connector connected, make these input tests at the connector. If a test indicates a problem, find and correct the cause, then recheck the system. If the input tests prove OK, replace the wipers/washers switch.
Cavity | Wire | Test condition | Test: Desired result | Possible cause if result is not obtained
--- | --- | --- | --- | ---
12 [9] | BLU/WHT | Ignition switch ON (II), the windshield wiper switch in ‘‘INT'' | Check for voltage between the No. 12 [No. 9] and No. 4 [No. 3] terminals: There should be about 0-5 V-0-5 V repeatedly. | Faulty wipers/washers switch Faulty windshield wiper motor An open in the wire
[ ]:RHD type except KE