## ABS Modulator-Control Unit Removal and Installation

NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water.
- Take care not to damage or deform the brake lines during removal and installation.
- To prevent the brake fluid from flowing, plug and cover the hose ends and joints with a shop towel or equivalent material.

## Removal

1. | Pull up the lock (A) of the ABS control unit 25P connector (B), and the connector disconnects itself.

2. | Disconnect the six brake lines.

3. | Remove the two 6 mm nuts.

4. | Remove the ABS modulator-control unit (C).

## Installation

1. | Install the ABS modulator-control unit, then tighten the two 6 mm nuts.

2. | Reconnect the six brake lines, then tighten the nuts.

3. | Align the connecting surface of the ABS control unit 25P connector.

4. | Push in the lock of the ABS control unit 25P connector until you hear it click into place, then connect the connector.

5. | Bleed the brake system, starting with the front wheels.

6. | Start the engine, and check that the ABS indicator goes off.

7. | Test-drive the vehicle, and check that the ABS indicator does not come on.