## Design Specifications

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
DIMENSIONS | Overall length |  | 3,830 mm (150.8 in.)
Overall width |  | 1,675 mm (65.9 in.)
Overall height |  | 1,525 mm (60.0 in.)
Wheelbase |  | 2,450 mm (96.5 in.)
Track equipped with 175 / 65 R14 82T tyres | Front | 1,460 mm (57.5 in.)
Rear | 1,445 mm (56.9 in.)
Track equipped with 185 / 55 R15 82V tyres | Front | 1,440 mm (56.7 in.)
Rear | 1,430 mm (56.3 in.)
Ground clearance |  | 140 mm (5.5 in.)
Seating capacity |  | four (4)
WEIGHT | Curb weight | M/T | 983-1,046kg (2,167-2,306 lbs)
CVT | 1,063-1,068kg (2,343-2,355 lbs)
Max. permissible weight (European models) | L12A1 engine | 1,470kg (3,241 lbs)
L13A1 engine | 1,490kg (3,285 lbs)
ENGINE | Type |  | Water-cooled, 4-stroke SOHC engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke | L12A1 engine | 73 x 74.4 mm (2.87 x 2.93 in.)
L13A1, L13A2 engines | 73 x 80 mm (2.87 x 3.15 in.)
Displacement | L12A1 engine | 1,246 cm3 (76 cu in.)
L13A1, L13A2 engines | 1,339 cm3 (82 cu in.)
Compression ratio |  | 10.8
Valve train |  | Chain drive, SOHC 2 valves per cylinder
Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | at 6,300 engine rpm (min-1) | 44.6 [liter] (47.1 US qt, 39.2 lmp qt)
Water pump displacement | at 6,000 engine rpm (min-1) | 120 [liter] (127 US qt, 106 lmp qt)
Fuel required | KE, KG, KR models | UNLEADED gasoline with 95 research octane number or higher
KK, KU models | UNLEADED gasoline with 91 research octane number or higher
STARTER | Type |  | Gear reduction
Normal output |  | 0.6 kW
Hour rating |  | 30 seconds
Rotation direction |  | Clockwise as viewed from gear end
CLUTCH | Clutch type | M/T | Single plate dry, diaphragm spring
CVT | Multi plates wet sump, hydraulic
Clutch friction material surface area | M/T | 136 cm2 (78.9 sq in.)

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
MANUAL TRANSMISSION | Type |  | Synchronized, 5-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio-L12A1 engine | 1st | 3.142
2nd | 1.750
3rd | 1.166
4th | 0.857
5th | 0.710
Reverse | 3.230
Final | 4.294
Gear ratio-L13A1 engine | 1st | 3.142
2nd | 1.750
3rd | 1.241
4th | 0.969
5th | 0.805
Reverse | 3.230
Final | 4.111
Final reduction | Type | Single helical gear
CVT | Type |  | Electronically controlled continuously variable transmission
Primary reduction |  | Direct 1:1
Gear ratio | Low-High | 2.367-0.407
Reverse | 2.367-1.326
Final reduction | Type | Single helical helical gear
Gear ratio | 4.333
STEERING | Type |  | Rack and pinion with electrical power-assisted
Overall ratio |  | 14.49
Turns, lock-to-lock |  | 2.83
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type | Front | Independent strut with stabilizer, coil spring
Rear | De Dion axle
Shock absorber | Front | Telescopic, hydraulic, nitrogen gas-filled
Rear | Telescopic, hydraulic, nitrogen gas-filled
WHEEL ALIGNMENT | Camber | Front | 0°
Rear | - 1°
Caster | Front | 2°10¢
Total toe | Front | 0 mm (0 in.)
Rear | In 2 mm (1/16 in.)
BRAKES | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid drum
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 44.5 cm2 (6.90 sq in.) x 2
Shoe friction surface area | Rear | 49.0 cm2 (7.60 sq in.) x 2
TYRES | Size of front and rear tyres |  | 175/65 R14 82T
| 185/55 R15 82V
Size of spare tyre |  | T115/70 D14 88M

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
AIR CONDITIONING | Compressor | Type | Scroll
Capacity | 85.7m[liter](5.23 cu in.) /rev.
Maximum speed | 12,000 rpm (min-1)
Lubricant capacity | 85m[liter] (2 1/6 fl oz)
Lubricant type | SP-10(KEIHIN)
Condenser | Type | Corrugated fin
Evaporator | Type | Corrugated fin
Blower | Type | Radial
Motor type | 220 W/12 V
Speed control | 4-speed
Maximum capacity | 380 m3/h (13,400 cu ft/h)
Temperature control |  | Air-mix type
Compressor clutch | Type | Dry, single plate, Poly V-belt drive
Electrical power consumption at 68°F (20°C) | 42 W maximum at 12 V
Refrigerant | Type | HFC-134 a (R-134 a)
Capacity | 400-450 g (14.1-15.9 oz)
ELECTRICAL RATINGS | Battery |  | 12 V-28 AH/5 hours
Starter |  | 12 V-0.6 kW
Alternator |  | 12 V-75 A
Fuses | Under-hood fuse/relay box | 80 A, 50 A, 40 A, 30 A, 20 A, 15 A, 10 A
Under-dash fuse/relay box | 20 A, 15 A, 10 A, 7.5 A
Light bulbs | Headlight high beam | 12 V-60 W
Headlight low beam | 12 V-55 W
Front turn signal/Front side marker lights | 12 V-21 W
Front parking lights | 12 V-5 W
Rear turn signal lights | 12 V-21 W
Brake/Taillights | 12 V-21/5 W
Back-up lights | 12 V-21 W
License plate light | 12 V-5 W
Ceiling light | 12 V-8 W
Tailgate light | 12 V-5 W
Spotlights | 12 V-5 W
Gauge lights | LED
Indicator lights | LED