## M/T Shift Lever Clearance Inspection

1. | Measure the clearance between shift lever (A) and the select lever (B) with a feeler gauge (C). If the clearance is more than the service limit, go to 2.
Standard: | 0.05 - 0.35 mm (0.002 - 0.014 in.)
Service Limit: | 0.55 mm (0.022 in.)

2. | Measure the groove of the shift lever. If distance is not within the standard, replace the shift lever with a new one. If distance is within the standard, replace the select lever with a new one.
Standard: | 13.00 - 13.15 mm (0.512 - 0.518 in.)