## CVT Drive Pulley Speed Sensor Replacement

1. | Disconnect the CVT drive pulley speed sensor connector.

2. | Remove the CVT drive pulley speed sensor.

3. | Install the new CVT drive pulley speed sensor (A) with the new O-ring (B). When installing the sensor, do not allow dust or other foreign particles to enter the transmission.

4. | Check the connector for rust, dirt, or oil, then connect the connector securely.