## Fuse Lid Assembly Removal/Installation

NOTE:

- Take care not to scratch the dashboard and related parts.
- LHD is shown, RHD is symmetrical.

1. | Remove the fuse lid (A) by pulling it back.

2. | Remove the screws (B, C), release the clips (D) and hooks (E) by pulling the driver's tray trim (F) back, then remove it.

3. | Install the trim and lid in the reverse order of reassembly. Push the clip and hook portions into place securely.