## Thermostat Replacement

## Removal:

1. | Remove the thermostat housing (A), then remove the thermostat (B).

## Installation:

1. | Remove old liquid gasket from the thermostat housing mating surfaces, bolts and bolt holes.

2. | Apply a 1.5 mm wide bead of the liquid gasket, P/N 08C70-K0234M, 08C70-K0334M or 08C70-X0331S, along the broken line (A). NOTE: Do not install the parts if 5 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue.

3. | Install the rubber seal (A) on the thermostat (B), then install the thermostat with the pin (C) up.

4. | Install the thermostat housing (D). NOTE: After assembly, wait at least 30 minutes before filling the engine with coolant.