## Tailgate Spoiler Replacement

## For Some Models

NOTE:

- Take care not to scratch the body.
- When prying component, use the handy remover set or equivalent.

1. | Remove the tailgate spoiler (A):
-1 | Pry up at the knotch (B) of the lid (C), then remove the lids from both sides.
-2 | Remove the bolts.
-3 | Lift the spoiler up, then remove it.

2. | Install the spoiler in the reverse order of removal. When installing, three locating bolts (D) should be fully inserted into grommets on the tailgate.