## ATF Strainer and Main Valve Body Removal

1. | Remove the ATF passage pipe (A).

2. | Remove the ATF strainer (B).

3. | Remove the ATF pass body (C), dowel pins (D), and separator plate (E).

4. | Remove the start clutch accumulator valve spring (F) and valve (G), then remove the main valve body (H) and dowel pins (I).

5. | Remove the ATF magnet (J), and clean it, then reinstall it in the flywheel housing (K).

6. | Replace the O-rings (L) with new ones, and install the all parts in the reverse order of removal.