## Windshield Wiper Blade Setting Position

## KQ model

1. | Pull up the wipers and activate them several times. NOTE: Please make sure to do this step in order to prevent the blades interference of driver's side and passenger's side.

2. | Return the wiper arm to the start position.

3. | Measure the distance from an edge of a cowl top to a wiper blade.
Driver side: | 50 mm
Passenger side: | 43 mm

4. | Remove the wiper arm and adjust the position if the measurements vary from the standard.

5. | Go back to 1 and 2 and confirm there is no interference of blades.