## DTC Troubleshooting: 62

DTC 62: | IG1 Voltage High

1. | Check the charging system. Is the charging system OK? YES - Go to 2. NO - Repair the charging system, then recheck.n

2. | Clear the DTCs using the HDS.

3. | Test-drive the vehicle at 15 km/h (9 mph) or more.

4. | Check the DTCs using the HDS. Does the ABS indicator come on, and are DTC 62 indicated? YES - Check for loose or poor connections in the VSA control unit 46P connector. If connections are good, replace the VSA modulator-control unit.n NO - The system is OK at this time.n