## Engine Oil Replacement

1. | Warm up the engine.

2. | Remove the drain bolt (A), and drain the engine oil.

3. | Reinstall the drain bolt with a new washer (B).

4. | Refill with the recommended oil.
Capacity
3.4 [liter] (3.6 US qt, 3.0 lmp qt) at oil change. 3.6 [liter] (3.8 US qt, 3.2 lmp qt) at oil change including filter. 4.2 [liter] (4.4 US qt, 3.7 lmp qt) after engine overhaul.

5. | Run the engine for more than 3 minutes, then check for oil leakage.