### Maintenance Schedule for Severe Conditions - Australia and New Zealand Models

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35°C (95°F) conditions.
- Extensive idling, or long periods of stop-and-go-driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 5,000 km (3,125 miles) or 6 months
Replace engine oil filter | Every 10,000 km (6,250 miles) or 6 months
Replace air cleaner element Use normal schedule except in dusty conditions. | l | l | l | l | l | l | l | l | l | l
Inspect valve clearance |  | l |  | l |  | l |  | l |  | l
Replace fuel filter |  | l |  | l |  | l |  | l |  | l
Replace spark plugs |  | l |  | l |  | l |  | l |  | l
Inspect and adjust drive belts Check for cracks, damage, deflection and tension |  | l |  | l |  | l |  | l |  | l
Inspect idle speed |  |  |  |  | l |  |  |  |  | l
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then replace every 100,000 km (60,000 miles) or 5 years
Replace manual transmission fluid (MTF) Use genuine Honda Manual Transmission Fluid MTF-II |  |  | l |  |  | l |  |  | l |
Replace CVT fluid (ATF) Use genuine Honda ATF-Z1 Replace every 40,000 km (25,000 miles) or 2 years, if the vehicle is driven under high speed driving in high temperature (over 35 °C/95 °F) condition. |  |  |  | l |  |  | l |  |  | l
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage and cracks brake pad, brake disc. Check the wheel cylinder for leaks Check the brake linings for cracking, glazing, wear and contamination Check the calipers for damage, leaks, and tightness | Every 10,000 km (6,250 miles) or 6 months
Replace brake fluid Use only DOT 3 brake fluid (We recommend Genuine Honda Brake Fluid). Check that brake fluid level between the upper and lower marks on the reservoir | Every 3 years

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Check parking brake adjustment | l | l |  | l |  | l |  | l |  | l
Check lights alignment Check the position of the headlights | l | l | l | l | l | l | l | l | l | l
Test drive (noise, stability, dashboard operation) Check for road stability, noise, vibration and dashboard operation. | l | l | l | l | l | l | l | l | l | l
Rotate tires Check tire inflation and condition at least once per month. | Every 10,000 km (6,250 miles)
Visually inspect the following items: Check for correct installation and position, check for cracks, deterioration, rust, and leaks. Check tightness of screws, nuts, and joints. If necessary, retighten.
Tie rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease | Every 10,000 km (6,250 miles) or 6 months
Suspension components Check the bolts for tightness. Check all dust cover for deterioration and damage.
Driveshaft boots Check the boot and boot band for cracks. Check rack grease.
Brake hoses and lines (including ABS) Check the master cylinder, proportioning control valve and ABS modulator and leakage | l | l | l | l | l | l | l | l | l | l
All fluid levels and condition of fluid Check levels and check for leaks. If necessary, add engine coolant, MTF, ATF, brake fluid, windshield fluid, and battery fluid.
Exhaust system Check the exhaust pipe and muffler for damage, leaks and tightness.
Fuel lines and connections Check fuel lines for loose connections, cracks and deterioration. Retighten loose connections and replace any damaged parts.